From f6d01996eb72fc71681efd4aacd8d8cb903be753 Mon Sep 17 00:00:00 2001
From: Loic Guegan <manzerberdes@gmx.com>
Date: Sat, 4 May 2019 10:32:19 +0200
Subject: Nix integration

---
 2019-Mascots.tex | 47 +++++++++++++++++++++++++++++------------------
 1 file changed, 29 insertions(+), 18 deletions(-)

(limited to '2019-Mascots.tex')

diff --git a/2019-Mascots.tex b/2019-Mascots.tex
index cd9243b..80d8f8b 100644
--- a/2019-Mascots.tex
+++ b/2019-Mascots.tex
@@ -36,38 +36,49 @@ component, formatting, style, styling, insert
 
 
 \section{Introduction}
-\label{sec:org9f2a447}
+\label{sec:org9428352}
 \section{Related Work}
-\label{sec:org3f89763}
+\label{sec:orga22ca2a}
 \section{Use-Case}
-\label{sec:org465840a}
+\label{sec:org3241664}
 \subsection{Application Characteristic}
-\label{sec:orgec764c1}
+\label{sec:org8ebb00c}
 \subsection{Cloud Infrastructure}
-\label{sec:orgd297b7a}
+\label{sec:org17d08e8}
 \section{System Model}
-\label{sec:orgb795527}
+\label{sec:org2051e46}
 \subsection{IoT Part}
-\label{sec:org2cfffb6}
+\label{sec:org9fc7024}
+The IoT part is composed of an Access Point (AP), connected to several sensors using WIFI. In the
+system, the IoT part is considered as the part where the system data are created. In fact, the
+data life cycle start when the sensors records their respectives local temperature at a frequency
+\(f\) and the local timestamp. Then, these data are transmitted through the network along with an
+arbitrary sensor id of 128 bits. Finally, the AP is in charge to transmit the data to the cloud
+using the network part.
+
 \subsection{Network Part}
-\label{sec:orgc144d77}
+\label{sec:orgb1e4614}
+The network part is considered as the medium that link the IoT part to the cloud. It is composed
+of several network switches and router and it is mostly considered as wired network.
+
+
 \subsection{Cloud Part}
-\label{sec:org39e083c}
+\label{sec:org4dad506}
 \section{Evaluation}
-\label{sec:org0d3d97d}
+\label{sec:org373c2b1}
 \subsection{IoT/Network Consumption}
-\label{sec:orgcb0df05}
-\subsection{Cloud Consmption}
-\label{sec:org4ed126a}
+\label{sec:org993439d}
+\subsection{Cloud Energy Consumption}
+\label{sec:org7ae8276}
 \subsection{Virtual Machine Size Impact}
-\label{sec:org9aec0d5}
+\label{sec:orgde03152}
 \subsection{Application Accuracy}
-\label{sec:org88409a4}
+\label{sec:org79ddac3}
 Refresh frequency etc\ldots{}
 \subsection{End-To-End Consumption}
-\label{sec:org1492f49}
+\label{sec:org275997a}
 \section{Discussion}
-\label{sec:org6627b27}
+\label{sec:org25eaadf}
 \section{Conclusion}
-\label{sec:org0643947}
+\label{sec:orgff11457}
 \end{document}
-- 
cgit v1.2.3

